X250

Objet : du tuto

Niveau requis :

Commentaires : Contexte d'utilisation du sujet du tuto.

Débutant, à savoir : Utiliser GNU/Linux en ligne de commande, tout commence là !.

Mise à jour BIOS

Installation de genisoimage :

apt install genisoimage

Création d'un dossier temporaire :

mkdir /tmp/x250_bios-update && cd /tmp/x250_bios-update

Récupérer le CD bootable contenant le BIOS :

read -p "Entrer l'URL du CD bootable : " isoURL # https://download.lenovo.com/pccbbs/mobiles/n10ur25w.iso read -p "Entrer le SHA256 du CD bootable : " isoSHA256 # e9a798ac9f964022f2b60c2269076b832ad19a6267e3729f8230335652f6309a wget $isoURL -O Bootable-CD.iso (sha256sum Bootable-CD.iso | grep $isoSHA256) && echo "Vérification OK" || echo "Vérification KO"

https://pcsupport.lenovo.com/fr/fr/products/laptops-and-netbooks/thinkpad-x-series-laptops/thinkpad-x250/20cl/20cls4mk00/pc084t5x/downloads/driver-list/component?name=BIOS

Extraire l'image du fichier ISO :

geteltorito -o bios.img Bootable-CD.iso

Copier l'image sur la clé USB :

dd if=bios.img of=/dev/sdz bs=64K status=progress && sync # Pour identifier la clé USB, utiliser lsblk

Redémarrer l'ordinateur :

systemctl reboot # as root

Mise à jour du BIOS depuis la clé USB :

Make sure your laptop power supply plugged in (he battery must charge to 80-100%)

interrupt boot process by pressing the ENTER key

hit the F12 key : Choose temporary startup device

select USB mass storage device as boot source

hit 2 : Update system program

Reconfigurer le BIOS :

Ressources : https://www.cyberciti.biz/faq/update-lenovo-bios-from-linux-usb-stick-pen/ https://wiki.archlinux.org/index.php/Lenovo_ThinkPad_X250#BIOS_updates